File Type: GeoTiff
Size is 6368, 5868

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (  94.9995824,  21.6755329) ( 94d59'58.50"E, 21d40'31.92"N)
Lower Left  (  94.9995824,  21.1661640) ( 94d59'58.50"E, 21d 9'58.19"N)
Upper Right (  95.5523535,  21.6755329) ( 95d33' 8.47"E, 21d40'31.92"N)
Lower Right (  95.5523535,  21.1661640) ( 95d33' 8.47"E, 21d 9'58.19"N)
Center      (  95.2759680,  21.4208484) ( 95d16'33.48"E, 21d25'15.05"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  ACQUISITION_DATETIME=2015:08:13 07:59:05
  ACQUISITION_DATETIME_TIMEZONE=GMT
  FIT_ERROR_RMS_PIXELS=12.1190744698
  POSITION_UNCERTAINTY_RMS_METERS=53.2288
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=projective
