File Type: GeoTiff
Size is 6902, 5875

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (-124.0778277,  41.3928987) (124d 4'40.18"W, 41d23'34.44"N)
Lower Left  (-124.0778277,  41.2343656) (124d 4'40.18"W, 41d14' 3.72"N)
Upper Right (-123.8915816,  41.3928987) (123d53'29.69"W, 41d23'34.44"N)
Lower Right (-123.8915816,  41.2343656) (123d53'29.69"W, 41d14' 3.72"N)
Center      (-123.9847046,  41.3136322) (123d59' 4.94"W, 41d18'49.08"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=5.65702452019
  POSITION_UNCERTAINTY_RMS_METERS=56.8018
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
