File Type: GeoTiff
Size is 6622, 5854

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (-122.3110440,  41.4826146) (122d18'39.76"W, 41d28'57.41"N)
Lower Left  (-122.3110440,  41.3106461) (122d18'39.76"W, 41d18'38.33"N)
Upper Right (-122.1165145,  41.4826146) (122d 6'59.45"W, 41d28'57.41"N)
Lower Right (-122.1165145,  41.3106461) (122d 6'59.45"W, 41d18'38.33"N)
Center      (-122.2137793,  41.3966304) (122d12'49.61"W, 41d23'47.87"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=7.17351810813
  POSITION_UNCERTAINTY_RMS_METERS=64.5263
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=projective
