File Type: GeoTiff
Size is 6682, 5850

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (-122.3131010,  41.4756645) (122d18'47.16"W, 41d28'32.39"N)
Lower Left  (-122.3131010,  41.3086587) (122d18'47.16"W, 41d18'31.17"N)
Upper Right (-122.1223432,  41.4756645) (122d 7'20.44"W, 41d28'32.39"N)
Lower Right (-122.1223432,  41.3086587) (122d 7'20.44"W, 41d18'31.17"N)
Center      (-122.2177221,  41.3921616) (122d13' 3.80"W, 41d23'31.78"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=39.7055393469
  POSITION_UNCERTAINTY_RMS_METERS=52.0792
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
