File Type: GeoTiff
Size is 7301, 5882

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (-122.1888893,  43.0110723) (122d11'20.00"W, 43d 0'39.86"N)
Lower Left  (-122.1888893,  42.8674638) (122d11'20.00"W, 42d52' 2.87"N)
Upper Right (-122.0106360,  43.0110723) (122d 0'38.29"W, 43d 0'39.86"N)
Lower Right (-122.0106360,  42.8674638) (122d 0'38.29"W, 42d52' 2.87"N)
Center      (-122.0997626,  42.9392681) (122d 5'59.15"W, 42d56'21.37"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=12.9741591224
  POSITION_UNCERTAINTY_RMS_METERS=51.5123
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
