File Type: GeoTiff
Size is 5721, 5126

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (  46.3116881,  32.5960838) ( 46d18'42.08"E, 32d35'45.90"N)
Lower Left  (  46.3116881,  32.1458090) ( 46d18'42.08"E, 32d 8'44.91"N)
Upper Right (  46.8142284,  32.5960838) ( 46d48'51.22"E, 32d35'45.90"N)
Lower Right (  46.8142284,  32.1458090) ( 46d48'51.22"E, 32d 8'44.91"N)
Center      (  46.5629582,  32.3709464) ( 46d33'46.65"E, 32d22'15.41"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=55.8125815418
  POSITION_UNCERTAINTY_RMS_METERS=45.2459
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
