File Type: GeoTiff
Size is 5633, 5274

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (  46.0469075,  32.6740370) ( 46d 2'48.87"E, 32d40'26.53"N)
Lower Left  (  46.0469075,  32.1761402) ( 46d 2'48.87"E, 32d10'34.10"N)
Upper Right (  46.5786961,  32.6740370) ( 46d34'43.31"E, 32d40'26.53"N)
Lower Right (  46.5786961,  32.1761402) ( 46d34'43.31"E, 32d10'34.10"N)
Center      (  46.3128018,  32.4250886) ( 46d18'46.09"E, 32d25'30.32"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=4.64876952246
  POSITION_UNCERTAINTY_RMS_METERS=44.9683
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
