File Type: GeoTiff
Size is 3280, 4872

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (    0.0,    0.0)
Lower Left  (    0.0, 4872.0)
Upper Right ( 3280.0,    0.0)
Lower Right ( 3280.0, 4872.0)
Center      ( 1640.0, 2436.0)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue

[Geographic Coordinate Information]
GCP Projection = 
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],

[Tie-Points Used For Georeferencing] {Point format is: (pixel column, pixel row) -> (longitude, latitude, 0)}
GCP[  0]: Id=1, Info=
          (634,2431.056818) -> (50.757866,15.102165,0)
GCP[  1]: Id=2, Info=
          (29,3596.659091) -> (50.876484,15.122456,0)
GCP[  2]: Id=3, Info=
          (1655,35.590909) -> (50.512991,15.042451,0)
GCP[  3]: Id=4, Info=
          (91,4758.306818) -> (50.964782,15.187645,0)
GCP[  4]: Id=5, Info=
          (1517,4642.636364) -> (50.899358,15.278389,0)
GCP[  5]: Id=6, Info=
          (2907,4795.875) -> (50.858717,15.381778,0)
GCP[  6]: Id=7, Info=
          (3192,3317.863636) -> (50.728769,15.327068,0)
GCP[  7]: Id=8, Info=
          (3182,2132.488636) -> (50.631866,15.265887,0)
GCP[  8]: Id=9, Info=
          (3168,80.079545) -> (50.455828,15.154406,0)
GCP[  9]: Id=10, Info=
          (2530,111.715909) -> (50.484023,15.109995,0)
GCP[ 10]: Id=11, Info=
          (1522,2462.693182) -> (50.724564,15.165217,0)
GCP[ 11]: Id=12, Info=
          (1486,3337.636364) -> (50.797069,15.209977,0)
GCP[ 12]: Id=13, Info=
          (1530,1643.113636) -> (50.655813,15.12259,0)

[Accuracy Measures For Georeferencing Result]
  ACQUISITION_DATETIME=2015:11:13 08:06:08
  ACQUISITION_DATETIME_TIMEZONE=GMT
  FIT_ERROR_RMS_PIXELS=33.8994190611
  POSITION_UNCERTAINTY_RMS_METERS=46.2692
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat

[Camera Metadata]
  EXIF_ApertureValue=(7.40088)
  EXIF_CFAPattern=0x2 00 0x2 00 00 0x1 0x1 0x2
  EXIF_ColorSpace=1
  EXIF_Contrast=0
  EXIF_CustomRendered=0
  EXIF_DateTime=2015:11:13 09:30:50
  EXIF_DateTimeDigitized=2015:11:13 08:06:08
  EXIF_DateTimeOriginal=2015:11:13 08:06:08
  EXIF_DigitalZoomRatio=(1)
  EXIF_ExifVersion=0221
  EXIF_ExposureBiasValue=(0)
  EXIF_ExposureMode=0
  EXIF_ExposureProgram=2
  EXIF_ExposureTime=(0.0015625)
  EXIF_FileSource=0x3
  EXIF_Flash=0
  EXIF_FNumber=(13)
  EXIF_FocalLength=(400)
  EXIF_FocalLengthIn35mmFilm=400
  EXIF_FocalPlaneResolutionUnit=3
  EXIF_FocalPlaneXResolution=(1368.89)
  EXIF_FocalPlaneYResolution=(1368.89)
  EXIF_GainControl=1
  EXIF_ISOSpeedRatings=400
  EXIF_LightSource=0
  EXIF_Make=NIKON CORPORATION
  EXIF_MaxApertureValue=(3)
  EXIF_MeteringMode=5
  EXIF_Model=NIKON D4
  EXIF_Orientation=1
  EXIF_PixelXDimension=3280
  EXIF_PixelYDimension=4928
  EXIF_ResolutionUnit=2
  EXIF_Saturation=0
  EXIF_SceneCaptureType=0
  EXIF_SceneType=0x1
  EXIF_SensingMethod=2
  EXIF_Sharpness=0
  EXIF_ShutterSpeedValue=(9.32193)
  EXIF_Software=Adobe Photoshop CC 2014 (Windows)
  EXIF_SubjectDistanceRange=0
  EXIF_SubSecTime=20
  EXIF_SubSecTime_Digitized=20
  EXIF_SubSecTime_Original=20
  EXIF_UserComment=NASA 2071124                   75.2F
  EXIF_WhiteBalance=0
  EXIF_XResolution=(300)
  EXIF_YResolution=(300)
