File Type: GeoTiff
Size is 4360, 5079

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -71.3755203, -32.3945911) ( 71d22'31.87"W, 32d23'40.53"S)
Lower Left  ( -71.3755203, -32.7865754) ( 71d22'31.87"W, 32d47'11.67"S)
Upper Right ( -71.0390265, -32.3945911) ( 71d 2'20.50"W, 32d23'40.53"S)
Lower Right ( -71.0390265, -32.7865754) ( 71d 2'20.50"W, 32d47'11.67"S)
Center      ( -71.2072734, -32.5905833) ( 71d12'26.18"W, 32d35'26.10"S)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=28.527165414
  POSITION_UNCERTAINTY_RMS_METERS=48.0532
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
