File Type: GeoTiff
Size is 4984, 5564

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -71.5468713, -32.5923385) ( 71d32'48.74"W, 32d35'32.42"S)
Lower Left  ( -71.5468713, -32.8457987) ( 71d32'48.74"W, 32d50'44.88"S)
Upper Right ( -71.3198322, -32.5923385) ( 71d19'11.40"W, 32d35'32.42"S)
Lower Right ( -71.3198322, -32.8457987) ( 71d19'11.40"W, 32d50'44.88"S)
Center      ( -71.4333517, -32.7190686) ( 71d26' 0.07"W, 32d43' 8.65"S)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=12.3994139484
  POSITION_UNCERTAINTY_RMS_METERS=46.2981
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
