File Type: GeoTiff
Size is 5838, 3959

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -92.1518433,  30.1666884) ( 92d 9' 6.64"W, 30d10' 0.08"N)
Lower Left  ( -92.1518433,  28.8601454) ( 92d 9' 6.64"W, 28d51'36.52"N)
Upper Right ( -90.2251956,  30.1666884) ( 90d13'30.70"W, 30d10' 0.08"N)
Lower Right ( -90.2251956,  28.8601454) ( 90d13'30.70"W, 28d51'36.52"N)
Center      ( -91.1885195,  29.5134169) ( 91d11'18.67"W, 29d30'48.30"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=21.927417529
  POSITION_UNCERTAINTY_RMS_METERS=61.9755
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
