File Type: GeoTiff
Size is 5808, 4258

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -92.1735481,  32.3245100) ( 92d10'24.77"W, 32d19'28.24"N)
Lower Left  ( -92.1735481,  31.3270808) ( 92d10'24.77"W, 31d19'37.49"N)
Upper Right ( -90.8130340,  32.3245100) ( 90d48'46.92"W, 32d19'28.24"N)
Lower Right ( -90.8130340,  31.3270808) ( 90d48'46.92"W, 31d19'37.49"N)
Center      ( -91.4932911,  31.8257954) ( 91d29'35.85"W, 31d49'32.86"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=27.9950269349
  POSITION_UNCERTAINTY_RMS_METERS=69.9127
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=projective
