File Type: GeoTiff
Size is 6483, 5425

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -90.2087943,  29.9924021) ( 90d12'31.66"W, 29d59'32.65"N)
Lower Left  ( -90.2087943,  28.7397463) ( 90d12'31.66"W, 28d44'23.09"N)
Upper Right ( -88.7118416,  29.9924021) ( 88d42'42.63"W, 29d59'32.65"N)
Lower Right ( -88.7118416,  28.7397463) ( 88d42'42.63"W, 28d44'23.09"N)
Center      ( -89.4603179,  29.3660742) ( 89d27'37.14"W, 29d21'57.87"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=14.4353026939
  POSITION_UNCERTAINTY_RMS_METERS=45.2656
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
