File Type: GeoTiff
Size is 6140, 4910

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -91.7194056,  30.0497173) ( 91d43' 9.86"W, 30d 2'58.98"N)
Lower Left  ( -91.7194056,  28.8718486) ( 91d43' 9.86"W, 28d52'18.65"N)
Upper Right ( -90.2464699,  30.0497173) ( 90d14'47.29"W, 30d 2'58.98"N)
Lower Right ( -90.2464699,  28.8718486) ( 90d14'47.29"W, 28d52'18.65"N)
Center      ( -90.9829378,  29.4607829) ( 90d58'58.58"W, 29d27'38.82"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  ACQUISITION_DATETIME=2016:08:17 17:18:10
  ACQUISITION_DATETIME_TIMEZONE=GMT
  FIT_ERROR_RMS_PIXELS=44.8082845806
  POSITION_UNCERTAINTY_RMS_METERS=42.2038
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
