File Type: GeoTiff
Size is 6106, 4604

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -92.4240725,  30.5338525) ( 92d25'26.66"W, 30d32' 1.87"N)
Lower Left  ( -92.4240725,  29.2480750) ( 92d25'26.66"W, 29d14'53.07"N)
Upper Right ( -90.7188254,  30.5338525) ( 90d43' 7.77"W, 30d32' 1.87"N)
Lower Right ( -90.7188254,  29.2480750) ( 90d43' 7.77"W, 29d14'53.07"N)
Center      ( -91.5714490,  29.8909638) ( 91d34'17.22"W, 29d53'27.47"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  FIT_ERROR_RMS_PIXELS=49.1494280942
  POSITION_UNCERTAINTY_RMS_METERS=46.3029
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
