File Type: GeoTiff
Size is 5635, 5565

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( -77.4095765,  26.8418636) ( 77d24'34.48"W, 26d50'30.71"N)
Lower Left  ( -77.4095765,  26.3422345) ( 77d24'34.48"W, 26d20'32.04"N)
Upper Right ( -76.9036627,  26.8418636) ( 76d54'13.19"W, 26d50'30.71"N)
Lower Right ( -76.9036627,  26.3422345) ( 76d54'13.19"W, 26d20'32.04"N)
Center      ( -77.1566196,  26.5920490) ( 77d 9'23.83"W, 26d35'31.38"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  ACQUISITION_DATETIME=2017:09:12 13:50:13
  ACQUISITION_DATETIME_TIMEZONE=GMT
  FIT_ERROR_RMS_PIXELS=2.8509251142
  POSITION_UNCERTAINTY_RMS_METERS=52.2624
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
