File Type: GeoTiff
       \\eo-web\ArcGIS\iss065\ISS065-E-220420\ISS065-E-220420.JPG.aux.xml

[Image Structure Metadata]
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  (-122.3163796,  42.0265743) (122d18'58.97"W, 42d 1'35.67"N)
Lower Left  (-122.3163796,  41.3188513) (122d18'58.97"W, 41d19' 7.86"N)
Upper Right (-121.4429952,  42.0265743) (121d26'34.78"W, 42d 1'35.67"N)
Lower Right (-121.4429952,  41.3188513) (121d26'34.78"W, 41d19' 7.86"N)
Center      (-121.8796874,  41.6727128) (121d52'46.87"W, 41d40'21.77"N)
Band 1 Block=128x128 Type=Byte, ColorInterp=Red
Band 2 Block=128x128 Type=Byte, ColorInterp=Green
Band 3 Block=128x128 Type=Byte, ColorInterp=Blue

[Geographic Coordinate Information]
GEOGCRS["WGS 84",
    DATUM["World Geodetic System 1984",
        ELLIPSOID["WGS 84",6378137,298.257223563,
            LENGTHUNIT["metre",1]]],
    PRIMEM["Greenwich",0,
        ANGLEUNIT["degree",0.0174532925199433]],
    CS[ellipsoidal,2],
        AXIS["geodetic latitude (Lat)",north,

[Accuracy Measures For Georeferencing Result]
  ACQUISITION_DATETIME=2021:08:04 20:59:36
  ACQUISITION_DATETIME_TIMEZONE=GMT
  FIT_ERROR_RMS_PIXELS=2.338797
  POSITION_UNCERTAINTY_RMS_METERS=37.42758289074532
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=Projective

