File Type: GeoTiff
Size is 4056, 3249

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( 139.9304812,  37.6623682) (139d55'49.73"E, 37d39'44.53"N)
Lower Left  ( 139.9304812,  37.3486976) (139d55'49.73"E, 37d20'55.31"N)
Upper Right ( 140.3220627,  37.6623682) (140d19'19.43"E, 37d39'44.53"N)
Lower Right ( 140.3220627,  37.3486976) (140d19'19.43"E, 37d20'55.31"N)
Center      ( 140.1262719,  37.5055329) (140d 7'34.58"E, 37d30'19.92"N)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  ACQUISITION_DATETIME=2014:04:16 06:44:44
  ACQUISITION_DATETIME_TIMEZONE=GMT
  FIT_ERROR_RMS_PIXELS=7.04568616238e-11
  POSITION_UNCERTAINTY_RMS_METERS=59.6248
  REGISTRATION_METHOD=Manual
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=projective
