File Type: GeoTiff
Size is 6465, 5502

[Image Structure Metadata]
  COMPRESSION=LZW
  INTERLEAVE=PIXEL
Corner Coordinates:
Upper Left  ( 120.3770039, -27.0735918) (120d22'37.21"E, 27d 4'24.93"S)
Lower Left  ( 120.3770039, -27.4287663) (120d22'37.21"E, 27d25'43.56"S)
Upper Right ( 120.7943436, -27.0735918) (120d47'39.64"E, 27d 4'24.93"S)
Lower Right ( 120.7943436, -27.4287663) (120d47'39.64"E, 27d25'43.56"S)
Center      ( 120.5856738, -27.2511791) (120d35' 8.43"E, 27d15' 4.24"S)
Band 1 Block=256x256 Type=Byte, ColorInterp=Red
  Mask Flags: PER_DATASET ALPHA 
Band 2 Block=256x256 Type=Byte, ColorInterp=Green
  Mask Flags: PER_DATASET ALPHA 
Band 3 Block=256x256 Type=Byte, ColorInterp=Blue
  Mask Flags: PER_DATASET ALPHA 
Band 4 Block=256x256 Type=Byte, ColorInterp=Alpha

[Geographic Coordinate Information]
GEOGCS["WGS 84",
    DATUM["WGS_1984",
        SPHEROID["WGS 84",6378137,298.257223563,
            AUTHORITY["EPSG","7030"]],
        AUTHORITY["EPSG","6326"]],
    PRIMEM["Greenwich",0],
    UNIT["degree",0.0174532925199433],
    AUTHORITY["EPSG","4326"]]

[Accuracy Measures For Georeferencing Result]
  ACQUISITION_DATETIME=2014:12:20 01:33:09
  ACQUISITION_DATETIME_TIMEZONE=GMT
  FIT_ERROR_RMS_PIXELS=4.33381114684
  POSITION_UNCERTAINTY_RMS_METERS=34.7007
  REGISTRATION_METHOD=Automated
  REGISTRATION_REFERENCE=Landsat
  RESAMPLING_METHOD=cubic
  WARP_TRANSFORM=quadratic
